* UDP has an 8-byte header



**IP fields used in pseudo-header**

* This pseudo header contains the following values from the IP header:
  + Source IP Address
  + Destination IP Address
  + Protocol value (PT)
  + UDP length (total length minus header length) == body length



